Term	Definitions	Acronym	
Accidental Emission
 	An unintended environmental release. 		
Allocation
 	Partitioning the input or output flows of a unit process to the product of interest. 		
Attributional Life Cycle Assessment
 	An LCA that accounts for flows/impacts of pollutants, resources, and exchanges among processes within a chosen temporal window. 	Attributional LCA 	
Background Data
 	The background data include energy and materials that are delivered to the foreground system as aggregated data sets in which individual plants and operations are not identified. 		
Brines (oilfield)
 	Wastewater produced along with crude oil and natural gas from oilfield operations. 		
By-Products
 	An incidental product deriving from a manufacturing process or chemical reaction, and not the primary product or service being produced. A by-product can be useful and marketable, or it can have negative ecological consequences. 		
Characterization
 	Characterization is the second step of an impact assessment and characterizes the magnitude of the potential impacts of each inventory flow to its corresponding environmental impact. 		
Characterization Factor
 	Factor derived from a characterization model which is applied to convert the assigned LCI results to the common unit of the category indicator. 		
Classification
 	Classification if the first step of an impact assessment and is the process of assigning inventory outputs into specific environmental impact categories. 		
Co-Product
 	A product produced together with another product. 		
Composite Data
 	Data from multiple facilities performing the same operation that have been combined or averaged in some manner. 		
Consequential Life Cycle Assessment
 	An LCA that attempts to account for flows/impacts that are caused beyond the immediate system in response to a change to the system. 	Consequential LCA 	
Environmental Aspects
 	Elements of a business' products, actions, or activities that may interact with the environment. 		
Environmental Loadings
 	Releases of pollutants to the environment, such as atmospheric and waterborne emissions and solid wastes. 		
Equivalency Factor
 	An indicator of the potential of each chemical to impact the given environmental impact category in comparison to the referenced chemical used. 		
Equivalent Usage Ratio
 	A basis for comparing two or more products that fulfill the same function. For example, comparing two containers based on a set volume of beverage to be delivered to the customer. 		
Facility-Specific Data
 	Data from a particular operation within a given facility that are not combined in any way. 		
Foreground Data
 	Data from the foreground system that is the system of primary concern to the analyst. 		
Fuel Processing and Delivery
 	Activities involved in the processing and delivery of fuel used to run a process; also Precombustion Energy. 	Fuel P&D 	
Functional Unit
 	The unit of comparison that assures that the products being compared provide an equivalent level of function or service. 		
Green Technology
 	A technology that offers a more environmentally benign approach compared to an existing technology. 		
Impact Assessment
 	The assessment of the environmental consequences of energy and natural resource consumption and waste releases associated with an actual or proposed action. 		
Impact Categories
 	Classifications of human health and environmental effects caused by a product throughout its life cycle. 		
Impact Indicators
 	Impact indicators measure the potential for an impact to occur rather than directly quantifying the actual impact. 		
Industrial System
 	A collection of operations that together perform some defined function. 		
Interpretation
 	The evaluation of the results of the inventory analysis and impact assessment to reduce environmental releases and resource use with a clear understanding of the uncertainty and the assumptions used to generate the results. 		
Inventory Analysis
 	The identification and quantification of energy, resource usage, and environmental emissions for a particular product, process, or activity. 		
Life Cycle Assessment
 	A cradle-to-grave approach for assessing industrial systems that evaluates all stages of a product's life. It provides a comprehensive view of the environmental aspects of the product or process. 		
Material Processing and Delivery
 	Activities involved in the processing and delivery of materials to a process. 	Material P&D 	
Normalization
 	Normalization is a technique for changing impact indicator values with differing units into a common, unitless format by dividing the value(s) by a selected reference quantity. This process increases the comparability of data among various impact categories. 		
Precombustion Energy
 	The extraction, transportation, and processing of fuels used for power generation, including adjusting for inefficiencies in power generation and transmission losses. 		
Product Life Cycle
 	The life cycle of a product system begins with the acquisition of raw materials and includes bulk material processing, engineered materials production, manufacture and assembly, use, retirement, and disposal of residuals produced in each stage. 		
Routine emissions
 	Those releases that normally occur from a process, as opposed to accidental releases that proceed from abnormal process conditions. 		
Sensitivity Analysis
 	A systematic evaluation process for describing the effect of variations of inputs to a system on the output. 		
Specific data
 	Data that are characteristic of a particular subsystem, or process. 		
Stressors
 	A set of conditions that may lead to an environmental impact. For example, an increase in greenhouse gases may lead to global warming. 		
System Flow Diagram
 	A depiction of the inputs and outputs of a system and how they are connected. 		
Weighting
 	The act of assigning subjective, value-based weighting factors to the different impact categories based on their perceived importance or relevance.