Term	Definitions	Acronym	
alpha particle
 	Alpha particles come from heavy radioactive elements such as uranium, radium and polonium. They can be stopped by a thin layer of light material, such as a sheet of paper, and cannot penetrate the outer, dead layer of skin. Therefore, they do not damage living tissue when outside the body. However, they can damage living tissue and pose a serious health threat if swallowed or inhaled. 		
ambient air
 	The air that surrounds us. 		
background radiation
 	Natural radiation caused by cosmic rays from space and radioactive elements found in the earth's crust. This natural radiation is around us at all times. 		
beta particles
 	Beta particles come from many different radioactive elements, both natural and man-made. Although they can be stopped by a thin sheet of aluminum, beta particles outside the body can cause burns to unprotected skin. They can pose a serious health threat if swallowed or inhaled. 		
composite sample
 	A sample formed by collecting several samples and combining them into a new sample for analysis. 		
counts per minute
 	The number of decays of radioactive material that are detected by a radiation detector in one minute. 	CPM 	
Curie
 	A measure of radioactivity based on the radioactive decay rate of one gram of radium-226. 	Ci 	
dose
 	Dose is defined as the amount of radiation or energy absorbed by a person's body. 		
fallout
 	Radioactive particles that fall to the ground after a nuclear explosion. 		
fixed monitor
 	Permanently positioned and continuously operating monitors that sample particulates in the air and obtain gamma radioactivity spectra in real-time. 		
gamma rays
 	Gamma rays come from many different radioactive elements, both natural and man-made. Gamma rays can easily pass completely through the human body, damaging tissue and DNA. Several inches of lead or a few feet of concrete may be required to stop gamma rays. 		
gamma spectroscopy
 	The analysis of photons (X-ray or Gamma) emitted from radioactive atoms as they undergo transformations to more stable atoms. The RadNet Fixed (Stationary) Monitors contain a detector system that provides information on the quantity and energy of photons emitted by radioactive material captured on the air filter (and the surroundings). These data may then be used by trained spectroscopists to identify the radioactive atoms that are emitting the gamma radiation. 		
gross
 	Total activity from all emitters (alpha or beta). 		
half-life
 	The time required for one half the atoms of a given amount of a radioactive isotope to radioactively decay. 		
ionizing radiation
 	Radiation with enough energy to remove electrons from atoms. 		
isotope
 	Isotopes are different versions of the same chemical element. Isotopes of an element have the same number of protons but a different number of neutrons. The number of neutrons determines the radioactivity of an element. 		
particulates
 	Tiny distinct particles such as dust that can be captured by filters from samples of air or water. 		
picocuries
 	One-trillionth (1/1,000,000,000,000) of a Curie. 	pCi 	
plume
 	An area of contamination as it spreads into the environment from its source. 		
radioactive decay
 	Spontaneous changes in the nucleus of an atom that produces ionizing radiation, including alpha or beta particles and/or gamma rays. 		
stationary monitor
 	Permanently positioned and continuously operating monitors that sample particulates in the air and obtain gamma radioactivity spectra in real-time.